## Color Coated Steel Coil(PPGI)

**Specification:**

|  |  |
| --- | --- |
| Product name | Pre-painted galvanized steel coil |
| Base material | hot dipped galvanized steel or Alu-Zic Steel |
| Standard | PPGI, SGCC, CGCC, DX51D, DC51D, TDC51D, TS280GP |
| Width | 700mm -1250mm (+/-0.02mm) |
| Thickness | 0.20 - 1.2mm (+/-0.15mm) |
| Zinc coating | 40g-2750g |
| Performance | Smooth or Matte or anti-scratch |
| Color | RAL COLOR,customized |
| Lacquer Coating thickness | according to customer needs |
| Certificate | ISO9001.ISO14001.OHSAS18001 |
| Application | Building industry ,structural use, roofing, commercial use ,household appliance,industry facilities,office buildings |
| Packing | Each coil packed with galvanized steel strip |
| Coil weight | 3--8 MT or as required |