**Welded Wire Mesh**

**Welded wire mesh** is welded form superior low carbon steel wire and then galvanized and PVC coated. It features smooth surface, uniform mesh, great corrosion resistance.

Welded wire mesh with excellent corrosion resistance and oxidation resistance, is extensively used as fencing, decoration and machinery protection material in agriculture, construction, transport, mine, sports field, lawn and various industrial fields.

**Specifications:**

Surface: Electro-galvanized, Hot dip galvanized, PVC coated welded mesh

|  |  |  |
| --- | --- | --- |
| **Welded Wire Mesh** | | |
| Opening | | Wire Diameter |
| In inch | In metric unit(mm) |
| 1/4" x 1/4" | 6.4mm x 6.4mm | 22,23,24 |
| 3/8" x 3/8" | 10.6mm x 10.6mm | 19,20,21,22 |
| 1/2" x 1/2" | 12.7mm x 12.7mm | 16,17,18,19,20,21,22,23 |
| 5/8" x 5/8" | 16mm x 16mm | 18,19,20,21, |
| 3/4" x 3/4" | 19.1mm x 19.1mm | 16,17,18,19,20,21 |
| 1" x 1/2" | 25.4mm x 12.7mm | 16,17,18,19,20,21 |
| 1-1/2" x 1-1/2" | 38mm x 38mm | 14,15,16,17,18,19 |
| 1" x 2" | 25.4mm x 50.8mm | 14,15,16 |
| 2" x 2" | 50.8mm x 50.8mm | 12,13,14,15,16 |
| Technical Note: 1,Standard roll length: 25m or 30m; Width: 0.5m to 2.0m 2,Other sizes available at request. 3,Packing: in waterproof paper in rolls or according to customer's request. | | |