**Seamless steel pipe**

Seamless steel belt for hollow sections, main used for transport liquid, for example ,petroleum, natural gas,water, gas and solid material.

**Applications:**

Low and middle pressure fluid pipeline, boiler, petroleum and natural gas industry, drilling, chemical industry, electric industry, shipbuilding, fertilizer equipment and pipeline, structure, petrochemical, pharmaceutical industry

**Advantages:**

1.High voltage-resistance

2.High Toughness

3.Short pipe length and less interface

**Specifications:**

|  |  |  |
| --- | --- | --- |
| Product Name: | Seamless steel pipe | |
| Size | OD | 12-1200mm |
|  | Wall Thickness | 1.5-100mm |
|  | Length | 5-12m |
| Steel material | A53B, A106B, API 5L GrB, SS400, Q235B, Q345B  ST37.0,ST35.8,St37.2,St35.4/8, S235 | |
| Usage | Used For Structure, Accessorize And Construction | |
| Surface Treatment | Black painting, varnish paint, anti rust oil, hot galvanized, cold galvanized, 3PE,etc.5) 3 PE, FBE, corrosion resistant coating | |
| Type | Seamless steel pipe | |
| Section Shape | Round | |
| Package | 1) In Bundle,  2) Clients' Requirements | |